K-Pod Release Notes

1.12	10/20/2021
 	Holding down F1 on power up, mutes beep. 
	Holding down F3 on power up, selects encoder 1:4 rate, 100 counts 		per revolution.
	Holding down F5 on power up, selects encoder 1:1 rate, 400 counts 		per revolution. 
	Holding down F6 on power up selects 1:0.5 rate, essentially 				doubles the count to 800 counts per revolution.
	Note: the K-Pod defaults to an encoder rate of 1:2 or 200 counts 			per revolution.  The encoder itself is capable of 400 counts per 		revolution.
	Encoder rates can now be configured via USB (for K4 use). 
		
1.11  06/29/2020
	Adds hold of F4 key on power-up selects 800 counts per revolution.

1.09	10/18/2016
	Changes encoder operation to allow the K-Pod to buffer  					encoder counts to the K3.  This helps the K3 and K-Pod remain
		in sync. 
	Adds a power-on feature: if the F3 button is held during power up
		the K-Pod encoder uses a divide by 4 scaling factor. 
	Adds configuration command to K-Pod USB interface. 

1.08	9/27/2016
	Adds ability to power K-Pod from a USB jack on a PC. 
	Added new USB commands which are documented in the K-Pod USB 		API spec.  

1.05	8/12/2016
	Adds LED and output control feature via K3 macros.  
	USB interface added which allows 3rd party programs access to K-			Pod via the USB generic HID specification.