KPA1500 Firmware Release Notes

03.07 11/14/2025

•	Add commands ^TX, ^RX, ^TQ to simulate pulling KEY IN down. See 3.07 update to KPA1500 Programing Reference.
•	Pause ATU tuning if forward power exceeds 100W to avoid switching ATU relays with too much exciter power. Display LCD message if this occurs.
•	LCD shows forward power if too low (< 5 W) or too high (> 100W) for ATU tuning to progress. Exciter foldback is common during ATU tune.
•	Switch VFWD/VREV to high power range if forward power exceeds 200W.