K-Pod Firmware Information

K-Pod MCU 1.09, 10/18/2016

Changes encoder operation to allow the K-Pod to buffer encoder counts to the K3.  This helps the K3 and K-Pod remain in sync. Adds a power-on feature: if the F3 button is held during power up the K-Pod encoder uses a divide by 4 scaling factor. Adds configuration command to K-Pod USB interface. 

K-Pod MCU 1.08, 9/27/2016
	
Adds ability to power K-Pod from a USB jack on a PC. Added new USB commands which are documented in the K-Pod USB API spec.  

K-Pod MCU 1.05, 8/12/2016
	
Adds LED and output control feature via K3 macros. USB interface added which allows 3rd party programs access to K-Pod via the USB generic HID specification.